# Specifying an IP address to be allowed to flood a VLAN using EDM

Use this procedure to configure the IP address multicast filter table. This table specifies multicast IP addresses that can be flooded to all ports on a per-VLAN basis.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. In the VLAN tree, double-click VLANs.

3. In the work area, click the IP Address Multicast Filter Table tab.

4. Click Insert

5. Complete the fields as required.

6. Click Insert

## Variable definitions

The following table describes the fields of the IP Address Multicast Filter Table tab.

Field | Definition
--- | ---
VlanAllowedInetAddressVlanId | Specifies the ID of the VLAN to configure.
VlanAllowedInetAddressType | Specifies the address type: ipv4.
VlanAllowedInetAddress | Specifies a multicast IP address that can flood all ports. You cannot specify unicast or broadcast addresses.