# Configuring Run IP Office using EDM

Use the following procedure to configure Run IP Office in automated or verbose mode.

## Procedure steps

1. From the navigation tree, double-click Administration.

2. In the Administration tree, double-click Run IP Office.

3. In the Automatic work area, type`1` to execute the script in the automated mode or type`2` to modify the predefined values in the Run Script Mode dialog box.

   If you type 1, the parameters are automatically configured. If you type 2, proceed with the following steps to modify the parameters in verbose mode.

4. In the Verbose work area, type the Voice VLAN ID in the Voice VLAN ID dialog box.

5. In the Voice VLAN Gateway IP Address dialog box, type the VLAN IP address.

6. In the Voice VLAN Gateway IP Mask dialog box, enter the VLAN IP mask address.

7. In the Data VLAN ID dialog box, type the data VLAN ID.

8. In the Data VLAN Gateway IP Address dialog box, type the data VLAN Gateway IP address.

9. In the IP Route to Gateway Modem-Router dialog box, type the IP route address to Gateway Modem-Router.

10. In the IP Office Call-Server IP Address dialog box, type the call server IP address.

11. In the IP Office File-Server IP Address dialog box, type the file server IP address.

12. Click Apply.

## Variable Definition

Variable | Value
--- | ---
Run Script Mode | Specifies to run the script either in automated or verbose mode.
Voice VLAN ID | Specifies the voice VLAN ID. By default, the voice VLAN ID is 42.
Voice VLAN Gateway IP Address | Specifies the Voice VLAN Gateway IP Address. By default, the voice VLAN gateway IP address is 192.168.42.254.
Voice VLAN Gateway IP Mask | Specifies the voice VLAN gateway IP mask address. By default, the voice VLAN gateway IP mask address is 255.255.255.0. The default subnet mask created by the run IP Office script supports a maximum of 250 hosts. You can change the subnet mask to 255.255.254.0 to allow 510 hosts for each subnet using the verbose mode.
Data VLAN ID | Specifies the data VLAN ID. By default, the data VLAN ID is 44.
IP Route to Gateway Modem-Router | Specifies the IP Route to gateway modem and router. By default, the IP address is 192.168.43.2.
IP Office Call-Server IP Address | Specifies the IP Office call server IP address. By default, the call server IP address is 192.168.42.1.
IP Office File-Server IP Address | Specifies the IP Office file server IP address. By default, the file server IP address is 192.168.42.1.