# Setting the C-BSR priority from the IP Routing menu

Use the following procedure to set the C-BSR priority on a VLAN from the IP Routing menu.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click PIM.

3. In the work area, click the Interfaces tab.

4. In the table, double-click the cell under the CBSRPreference column heading for the parameter you want to change.

5. Type the value of the C-BSR priority for the associated interface.

   The Candidate BSR with the highest BSR-priority and address is the preferred BSR. The default is –1, which indicates that the current interface is not a Candidate BSR; the range is 0 to 255.

6. In the toolbar, click Apply.