# Viewing LLDP remote properties

Use this procedure view LLDP properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Neighbor tab.

The following table outlines the parameters of the Neighbor tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry. See the TimeFilter textual convention in IETF RFC 2021 for details about TimeFilter.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Specifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
ChassisIdSubtype | Specifies the type of encoding used to identify the remote system chassis: chassisComponent interfaceAlias portComponent macAddress networkAddress interfaceName local.
ChassisId | Specifies the remote chassis ID.
SysCapSupported | Identifies the system capabilities supported on the remote system.
SysCapEnabled | Identifies the system capabilities that are enabled on the remote system.
SysName | Specifies the remote system name.
SysDesc | Specifies the remote system description.
PortIdSubtype | Specifies the type of encoding used to identify the remote port. interfaceAlias portComponent macAddress networkAddress interfaceName agentCircuitId local
PortId | Specifies the remote port ID.
PortDesc | Specifies the remote port description.