# Viewing LLDP protocol VLAN properties

Use this procedure to view LLDP Protocol VLAN properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Local Protocol VLAN tab.

The following table outlines the parameters of the Local Protocol VLAN tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
ProtoVlanId | Specifies the ID of the port and protocol VLANs associated with the local port. A value of zero is used if the system does not know the protocol VLAN ID (PPVID).
ProtoVlanSuported | Indicates whether the local port supports port and protocol VLANs.
ProtoVlanEnabled | Indicates whether the port and protocol VLANs are enabled on the local port.
ProtoVlanTxEnable | Indicates whether the corresponding local port and protocol VLAN information are transmitted from the port.