# Configuring the IPv4 remote access list

Use this procedure to configure a list of IPv4 source addresses for which to permit remote access to a switch.

## Procedure steps

1. From the navigation tree, double-click Administration.

2. In the Administration tree, double-click Remote Access.

3. In the work area, click the Allowed List(IPv4) tab.

4. To select a source to edit, click the source row.

5. In the source row double-click the cell in the Allowed Source IP Address column.

6. In the dialog box, type a value.

7. In the source rowdouble-click the cell in the Allowed Source Mask column.

8. In the dialog box, type a value.

9. Click Apply.

Use the data in this table to configure to configure a list of IPv4 source addresses for which to permit access to the switch.

Table 1. Variable definitions
Variable | Value
--- | ---
Allowed Source IP Address | Specifies the source IPv4 address to permit remote access to the switch.
Allowed Source Mask | Specifies subnet mask associated with the source IPv4 address to permit remote access to the switch.