# Viewing LLDP link aggregation properties

Use this procedure to view LLDP link aggregation properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local Link Aggregate tab.

The following table outlines the parameters of the Port dot3 Local Link Aggregate tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
LinkAggStatus | Specifies the link aggregation capabilities and the current aggregation status of the link.
LinkAggPortId | Contains the IEEE 802.3 aggregated port identifier, aAggPortID (IEEE 802.3-2002, 30.7.2.1.1), derived from the ifNumber of the ifIndex for the port component in link aggregation. If the port is not in a link aggregation state or does not support link aggregation, this value is set to zero.