# Deleting a CLIP interface

Use this procedure to delete CLIP from a loopback interface.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click IP.

3. In the IP work area, click the Circuitless IP tab.

4. In the Circuitless IP work area, click the IfIndex of the CLIP to delete.

5. On the toolbar, click Delete.

6. On the toolbar, click Refresh to verify the CLIP interface is deleted from the system.