# Viewing LLDP management properites

Use this procedure to view LLDP management properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Local Management tab.

The following table outlines the parameters of the Local Management tab.

Table 1. Variable definitions
Variable | Value
--- | ---
AddrSubtype | Specifies the type of management address identifier encoding used in the associated Addr object.
Addr | Specifies the string value used to identify the management address component associated with the local system. This address is used to contact the management entity.
AddrLen | Specifies the total length of the management address subtype and the management address fields in LLDPDUs transmitted by the local LLDP agent. The management address length field is needed so that the receiving systems that do not implement SNMP are not required to implement an iana family numbers/address length equivalency table to decode the management address.
AddrIfSubtype | Identifies the numbering method used to define the interface number associated with the remote system. unknown ifIndex systemPortNumber
AddrIfId | Identifies the interface number of the management address component associated with the local system.
AddrOID | Identifies the type of hardware component or protocol entity associated with the management address advertised by the local system agent.
AddrPortsTxEnable | Identifies the ports on which the local system management address TLVs are transmitted in the LLPDUs.