# Configuring QoS for the NSNA solution using EDM

Use the following procedure to configure QoS for the NSNA solution using EDM.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

For general information about configuring filters and Quality of Service (QoS) in the NSNA solution, see Filters in the NSNA solution in Configuration — Security Avaya Ethernet Routing Switch 5000 Series (NN47200-501).

For detailed information about configuring the filters, see Avaya Ethernet Routing Switch 5000 Series Configuration — Quality of Service (NN47200-504).