# Configuring the switch file server IP address TLV

Use this procedure to define the local file server IP addresses that switch ports can advertise to Avaya IP phones.

You can define IP addresses for a maximum of 4 local call servers.

Note

If your Avaya IP Handset uses SIP, 802.1AB (LLDP) TLVs do not provide all information for the IP Phone. You must specify a file server IP address TLV so the IP phone can download the SIP configuration information, because the IP Phone retrieves information related to the SIP domain, port number and transport protocol from the file server.

Important

The switch does not support the advertisement of IPv6 addresses to Avaya IP phones.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, click Diagnostics.

3. In the Diagnostics tree, click 802.1AB.

4. In the 802.1AB tree, click Avaya.

5. In the Avaya work area, click the Local File Servers tab.

6. Click FileServerNum to select a port.

7. In the port row, configure as required.

8. On the toolbar, click Apply.

9. On the toolbar, you can click Refresh to verify the configuration.

## Variable definitions

The following table describes the variables associated with the Local File Servers tab

Variable | Value
--- | ---
FileServerNum | Displays the file server number.
FileServerAddressType | Displays the file server IP address type.
FileServerAddress | Defines file server IP address to advertise.