# Displaying the current BSR

Use the following procedure to display the current BSR information to review the configuration.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click PIM.

3. In the work area, click the Current BSR tab to view the current BSR information.

## Variable definitions

The following table describes the fields of the Current BSR tab.

Field | Description
--- | ---
Address | Specifies the IP address of the current BSR for the local PIM domain.
FragmentTag | Specifies a randomly generated number that distinguishes fragments belonging to different bootstrap messages. Fragments belonging to the same bootstrap message carry the same Fragment Tag.
HashMask | Specifies the mask used in the hash function to map a group to one of the C-RPs from the RP set. With the hash mask, a small number of consecutive groups can always hash to the same RP.
Priority | Specifies the priority of the current BSR. The candidate BSR (C-BSR) with the highest BSR priority, and address (referred to as the preferred BSR) is elected as the BSR for the domain.
BootStrapTimer | Specifies the interval (in seconds) that the elected BSR waits between originating bootstrap messages.