# Viewing traffic profile sets

Use this procedure to open the Set tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS NSNA/UBP/Traffic Profile.

3. Select the Set tab.

## Variable definitions

The following table outlines the parameters of the Set tab.

Table 1. QoS NSNA/UBP/Traffic Profile Set tab parameters
Variable | Value
--- | ---
AclType | Specifies the type of ACL (NSNA, UBP, or Traffic Profile).
Name | Specifies a name for this entry. The name must be an existing classifier name. All classifiers with this name are part of this filter set. The filter set itself has this name.
IfIndex | Specifies the logical interface index assigned to the VLAN or the physical interface.
MeteringMode | Specifies the Traffic Profile Metering Mode as: noMetering perPolicyUniformRateMetering perPolicyIndividualRateMetring perClassifierMetering
CommittedRate | Specifies the committed rate (in Kbps).
BurstSize | Specifies the maximum number of bytes in a single transmission burst.
OutActionDrop | Specifies the action to take when packet is out-of-profile. This action is applied only if metering is being enforced, and if the traffic is deemed out-of-profile based on the level of traffic and the metering criteria. (Metering is applied only to traffic matching the filtering data.) Options are the following: drop (packet is dropped) pass (packet is not dropped)
OutActionUpdateDscp | Specifies the action to take to update DSCP when a packet is out-of-profile. The default value is -1. The value range is between -1–63.
SetPriority | Specifies the priority in the range 1–255. You can only change this field for a User Based Policy set. .
Status | Enables or disables the Traffic Profile set policy.
Storage | Specifies the type of storage for this entry.

This section contains information about the following topics:

- Configuring a set

- Deleting a set

- Filtering a set