# Run IP Office script Configuration

The Run IP Office script executes a set of commands in either a fully automated or user prompted configuration on ACLI or EDM. In a fully automated or non-verbose mode, the scripts are executed with the predefined default values. In a user-prompted or the verbose mode, you can use the script to modify the default values.

You do not need access rights to execute the script. The script is available in both standalone and stacking mode. In stacking mode, you must execute the script from the base unit.

Note

The script must be executed on a switch with default settings. If you execute the script on a switch that is already configured, you can encounter script failure or an incomplete configuration.

Table 1. Default parameters for Run IP Office script
Voice VLAN ID | 42
Voice VLAN 42 gateway IP | 192.168.42.254
Data VLAN ID | 44
Data VLAN 44 gateway IP | 192.168.44.254
Data VLAN Gateway IP/mask | 255.255.255.0
IP Route to Gateway Modem-Router (Internet/WAN) | 192.168.43.2
IP Office Call server address | 192.168.42.1
IP Office File server address | 192.168.42.1
Switch port 1 (or 1/1) | IP Office
Switch port 2 (or 1/2) | Gateway Modem-Router port