# Configuring ADAC settings

Use this procedure to configure the global ADAC settings.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Chassis.

3. From the Chassis tree, click ADAC.

4. Select the ADAC tab.

5. Select the AdminEnable field to enable ADAC.

6. Choose the Operating Mode.

7. In the NotificationControlEnable field, enable or disable trap notifications.

8. Enter the Voice VLAN ID, Call Server port, and Uplink port.

9. Click Apply.

## Variable definitions

The following table outlines the parameters of the ADAC tab.

Table 1. ADAC tab parameters
Variable | Value
--- | ---
AdminEnable | Enables and disables ADAC.
OperEnable | Indicates ADAC operational state: true is enabled and false is disabled. Note If AdminEnable is True and OperEnable is False, this indicates an error condition such as missing Uplink and Call Server ports.
OperatingMode | Sets the ADAC operation mode: untaggedFramesBasic: IP Phones send untagged frames, and the Voice VLAN is not created. untaggedFramesAdvanced: IP Phones send untagged frames, and the Voice VLAN is created. taggedFrames: IP Phones send tagged frames.
NotificationControlEnable | Enables and disables ADAC trap notifications.
VoiceVLAN | Sets the Voice VLAN ID.
CallServerPort | Sets the Call Server port. The Ethernet Routing Switch 5000 Series supports up to 8 Call Server ports.
UplinkPort | Sets the Uplink port. The Ethernet Routing Switch 5000 Series supports up to 8 Uplink ports.
MacAddrRangeControl | Provides two options for configuring the MAC address range table: clearTable: clears the MAC address range table. defaultTable: sets the MAC address range table to its default values.