# Configuring the IPv6 remote access list using EDM

Use this procedure to configure a list of IPv6 source addresses for which to permit remote access to a switch.

## Procedure steps

1. From the navigation tree, double-click Administration.

2. In the Administration tree, double-click Remote Access .

3. In the work area, click the Allowed List(IPv6) tab.

4. To select a source to edit, click the source row.

5. In the source rowdouble-click the cell in the Allowed Source IPv6 Address column.

6. In the dialog box, type a value.

7. In the source row, double-click the cell in the Allowed Prefix Length column.

8. In the dialog box, type a value.

9. Click Apply.

Use the data in this table to configure to configure a list of IPv6 source addresses for which to permit access to the switch .

Table 1. Variable definitions
Variable | Value
--- | ---
Allowed Source IPv6 Address | Specifies the source IPv6 address to permit remote access to the switch.
Allowed Prefix Length | Specifies prefix length for the source IPv6 address to permit remote access to the switch. Values range from 0 to 128.