# Viewing LLDP neighbor PoE properties

Use this procedure to view LLDP PoE properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Neighbor PoE tab.

The following table outlines the parameters of the Port dot3 Neighbor PoE tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Indicates the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Identifies a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
PowerPortClass | Identifies the port Class of the remote port.
PowerMDISupported | Indicates whether MDI power is supported on the remote port.
PowerMDIEnabled | Indicates whether MDI power is enabled on the remote port.
PowerPairControlable | Indicates whether pair selection can be controlled on the remote port, derived from the value of the pethPsePortPowerPairsControlAbility object (defined in IETF RFC 3621).
PowerPairs | Contains the value of the pethPsePortPowerPairs object (defined in IETF RFC 3621) for the remote port. signal spare
PowerClass | Contains the value of the pethPsePortPowerClassifications object (defined in IETF RFC 3621) for the remote port. class0 class1 class2 class3 class4