# Viewing port non-EAP host support status using EDM

Use the following procedure to display the status of non-EAP host support on the port.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

   The Port tab appears.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Non-EAP MACHost.

   The Non-EAP MAC, Port tab appears.

6. In the work area, click the Non-EAP Status tab

## Variable definitions

Use the data in the following table to view port non-EAP host support status.

Variable | Value
--- | ---
PortNumber | Specifies the port number in use.
ClientMACAddr | Specifies the MAC address of the client.
State | Specifies the authentication status. Possible values are: rejected: the MAC address cannot be authenticated on this port. locallyAuthenticated: the MAC address was authenticated using the local table of allowed clients. radiusPending: the MAC address is awaiting authentication by a RADIUS server. radiusAuthenticated: the MAC address was authenticated by a RADIUS server. adacAuthenticated: the MAC address was authenticated using ADAC configuration tables. mhsaAuthenticated: the MAC address was auto-authenticated on a port following successful. authentication of an EAP client.
Reauthenticate | Specifies the value used to reauthenticate the MAC address of the client on the port.