# Displaying the PoE information for a unit

Use this procedure to display PoE information for a single unit.

Note

You can only view PoE parameters by selecting a single unit.

## Procedure

1. In the Device Physical View, select the unit.
2. From the navigation tree, double-click Edit.
3. From the Edit tree, click Unit.
4. Select the PoE tab.

## PoE field descriptions

The following table outlines the parameters of the PoE tab.

Name | Description
--- | ---
Power | Displays the total power available to the Avaya Ethernet Routing Switch.
OperStatus | Displays the power state of the Avaya Ethernet Routing Switch on off faulty
Consumption Power | Displays the power being used by the Avaya Ethernet Routing Switch.
UsageThreshold | Enables you to set a percentage of the total power usage of the Avaya Ethernet ROouting Switch based on which system sends a trap. Note You must have the traps enabled (see NotificationControlEnable) to receive a power usage trap.
Notification Control Enable | Enables you to enable or disable sending traps if the switch's power usage exceeds the percentage set in the Usage Threshold field.
PowerDeviceDetectType | Enables you to set the power detection method that the switch uses to detect a request for power from a device connected to all ports on the switch: 802.3af. 802.3afAndLegacySupport