# Displaying VLAN configuration

Use this procedure to display basic VLAN configuration

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click VLANs.

3. Select the Basic tab.

Variable definitions

The following table outlines the parameters of the Basic tab.

Table 1. VLAN Basic tab parameters
Variable | Value
--- | ---
Id | The VLAN ID for the VLAN.
Name | Name of the VLAN.
Ifindex | Indicates the interface index.
Type | Indicates the type of VLAN: byPort or byProtocolId.
VoiceEnabled | Indicates whether VLAN is a voice VLAN (true) or not (false).
PortMembers | Ports that are members of the VLAN.
ActiveMembers | Set of ports that are currently active in the VLAN. Active ports include all static ports and any dynamic ports where the VLAN policy was met.
StgId | Identifies the spanning tree group to which the VLAN belongs. This field is only available when the switch is running in Avaya STPG mode.
VrfId | Identifies the numerical ID for the VRF instance. Value ranges from 0 to 3.
VrfName | Identifies the alphanumeric identifier (name) assigned to the VRF instance.
MstpInstance | This field is only available when the switch is running in MSTP mode.
ProtocolId | Protocol for protocol-based VLANs. This value is taken from the Assigned Numbers RFC. For port-based VLANs, None is the displayed value.
UserDefinedPid | When rcVlanProtocolId is set to usrDefined(15) in a protocol-based VLAN, this field represents the 16-bit user-defined protocol identifier.
Encap | The type of encapsulation. Options are ethernet2 and llc.
MacAddress | The unique hardware address of the device.
Routing | Specifies whether routing is enabled (true) or disabled (false) on the VLAN.