# Viewing LLDP neighbor location properties

Use this procedure to view LLDP location properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Neighbor Location tab.

The following table outlines the parameters of the Port MED Neighbor Location tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Identifies a particular MSAP, using an arbitrary local integer value. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
LocationSubtype | Identifies the location subtype advertised by the remote device: unknown coordinateBased civicAddress elin
LocationInfo | Specifies the location information advertised by the remote device. The parsing of this information is dependent on the location subtype.