# Viewing LLDP VLAN Name properties

Use this procedure to view LLDP VLAN Name properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Local VLAN Name tab.

The following table outlines the parameters of the Local VLAN Name tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
VlanId | Specifies the integer value used to identify the IEEE 802.1Q VLAN IDs with which the given port is compatible.
VlanName | Indicates the string value used to identify the VLAN name identified by the VLAN ID associated with the given port on the local system. This object contains the value of the dot1QVLANStaticName object (defined in IETF RFC 2674) identified with the given lldpXdot1LocVlanId.
VlanNameTxEnable | Indicates whether the corresponding Local System VLAN name instance is transmitted from the port.