# Graphing the EAPOL Stats tab using EDM

Use the following procedure to view read-only EAPOL statistics.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

1. In the Device Physical View, select one or multiple ports.

2. From the navigation tree, double-click Graph.

3. In the Graph tree, double-click Port.

4. In the work area, click the EAPOL Stats tab to view information about EAPOL statistics.

## Variable definitions

The following table describes the fields of EAPOL Stats tab.

Field | Description
--- | ---
EapolFramesRx | Indicates the number of valid EAPOL frames that have been received by this authenticator.
EapolFramesTx | Indicates the number of EAPOL frame types that have been transmitted by this authenticator.
EapolStartFramesRx | Indicates the number of EAPOL start frames that have been received by this authenticator.
EapolLogoffFramesRx | Indicates the number of EAPOL Logoff frames that have been received by this authenticator.
EapolRespIdFramesRx | Indicates the number of EAPOL Resp/Id frames that have been received by this authenticator.
EapolRespFramesRx | Indicates the number of valid EAP Response frames (other than Resp/Id frames) that have been received by this authenticator.
EapolReqIdFramesTx | Indicates the number of EAPOL Req/Id frames that have been transmitted by this authenticator.
EapolReqFramesTx | Indicates the number of EAP Req/Id frames (Other than Rq/Id frames) that have been transmitted by this authenticator.
InvalidEapolFramesRx | Indicates the number of EAPOL frames that have been received by this authenticator in which the frame type is not recognized.
EapLengthErrorFramesRx | Indicates the number of EAPOL frames that have been received by this authenticator in which the packet body length field is not valid.