# Editing LLDP MED policies

Use this procedure to edit a previously configured LLDP MED policy for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Diagnostics.

3. In the Diagnostic tree, double-click 802.1AB.

4. In the 802.1AB tree, double-click Port MED.

5. To select a policy to edit, click the PortNum.

6. In the policy row, double-click the cell in thePolicyVlanID column.

7. Select a VLAN from the list.

8. Click Ok .

9. In the policy row, double-click the cell in thePolicyPriority column.

10. Edit the policy priority value.

11. In the policy row, double-click the cell in thePolicyDscp column.

12. Edit the policy DSCP value.

13. In the policy row, double-click the cell in thePolicyTagged column.

14. Select a value from the list.

15. On the toolbar, click Apply .

Use the data in the following table to edit a previously configured LLDP MED policy for the local system.

Table 1. Variable definitions
Field | Description
--- | ---
PortNum | Indicates the port on which to configure LLDP MED policies. This is a read-only cell.
PolicyAppType | Indicates the policy application type. This is a read-only cell. voice— voice network policy voiceSignaling— voice signaling network policy
PolicyVlanID | Specifies the VLAN identifier for the selected port or ports. Values range from 1–4094. If you select priority tagged frames, the system recognizes only the 802.1p priority level and uses a value of 0 for the VLAN ID of the ingress port.
PolicyPriority | Specifies the value of the 802.1p priority that applies to the selected switch port or ports. Values range from 0–7.
PolicyDscp | Specifies the value of the Differentiated Service Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475 that is associated with the selected switch port or ports. Values range from 0–63.
PolicyTagged | Specifies the type of VLAN tagging to apply on the selected switch port or ports. true—uses a tagged VLAN false—uses an untagged VLAN or does not support port-based VLANs. If you select untagged, the system ignores the VLAN ID and priority values, and recognizes only the DSCP value.