# Configuring the NEAP RADIUS server using EDM

Use this procedure to configure a Non-EAP (NEAP) RADIUS Server for processing NEAP client requests only.

## Procedure

1. From the navigation tree, double-click Security.
2. In the Security tree, click RADIUS.
3. In the RADIUS work area, click the NEAP RADIUS Server tab.
4. In the NEAP RADIUS Server section, configure as required.
5. On the toolbar, click Apply.
6. On the toolbar, you can click Refresh to verify the configuration.

## Variable definitions

Variable | Value
--- | ---
PrimaryRadiusServerAddressType | Specifies the type of IP address type for the primary NEAP RADIUS server. Values include unknown, ipv4, and ipv6.
PrimaryRadiusServer | Specifies the IPv4 or IPv6 address for the primary NEAP RADIUS Server. The default address is 0.0.0.0. Important: Important An IPv4 address value of 0.0.0.0 indicates that a primary NEAP RADIUS Server is not configured. An IPv6 value of 00:00:00:00:00:00:00:00 indicates that a primary NEAP RADIUS server is not configured.
SecondaryRadiusServerAddressType | Specifies the IP address type for the secondary NEAP RADIUS Server. Values include unknown, ipv4, and ipv6.
SecondaryRadiusServer | Specifies the IP address for the secondary NEAP RADIUS Server. The default address is 0.0.0.0. The secondary NEAP RADIUS Server is used only if the primary NEAP RADIUS Server is unavailable or unreachable. Important An IPv4 address value of 0.0.0.0 indicates that a secondary NEAP RADIUS Server is not configured. An IPv6 value of 00:00:00:00:00:00:00:00 indicates that a secondary NEAP RADIUS server is not configured.
RadiusServerUdpPort | Specifies the UDP port number for clients to use when trying to contact the NEAP RADIUS Server at the corresponding NEAP RADIUS Server IP address. Values range from 1 to 65535. The default port number is 1812.
RadiusServerTimeout | Specifies the timeout interval between each retry for service requests to the NEAP RADIUS Server. The default is 2 Seconds. Values range from 1 to 60 seconds.
SharedSecret(Key) | Specifies a new value for the NEAP RADIUS Server shared secret key, to a maximum of 16 characters.
ConfirmedSharedSecret(key) | Confirms the value typed in the shared secret key box. If you do not change the NEAP RADIUS Server shared secret key, you do not have to type a value in this box.
AccountingEnabled | Enables or disables RADIUS accounting for a NEAP RADIUS Server instance.
AccountingPort | Specifies the UDP accounting port number for clients to use when trying to contact the NEAP RADIUS Server at the corresponding NEAP RADIUS Server IP address. Values range from 0 to 65535.
RetryLimit | Specifies the number of RADIUS retry attempts for a NEAP RADIUS Server instance. Values range from 1 to 5.