# Viewing BGP summary route information

Use the following procedure to display current BGP route information.

## Procedure

1. In the navigation tree, open the following folders: Configuration > IP.
2. Click BGP.
3. Click the Bgp Route Summary tab.

## Bgp Route Summary field descriptions

Use the data in the following table to use the Bgp Route Summarytab.

Name | Description
--- | ---
Prefix | Specifies the IP address prefix in the Network Layer Reachability Information (NLRI) field. This is an IP address that contains the prefix with a length specified by IpAddrPrefixLen. Any bits beyond the length specified by IpAddrPrefixLen are set to zero.
PrefixLen | Specifies the length, in bits, of the IP address prefix in the NLRI field.
LocalAddr | The local address of this entry's BGP connection.
RemoteAddr | Specifies the IP address of the peer from which path information was learned.