                    GRAY RAMP


This gray ramp pattern can be used to check color
balance and to adjust the white level.

You should make sure the bars are gray, with no
red or blue bias. This can be adjusted with the
individual color settings, or the tint control
in NTSC displays.
