                Memory Viewer

This shows selected regions of the main CPU memory
map.

The current address range is shown in red at the
right from top to bottom.

The left part of the screen shows 0x1C0 bytes in
hex.

- Button I toggles ASCII mode.
