#N canvas 363 399 572 344 10;
#X obj 80 170 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X floatatom 80 220 5 0 0 0 - - -;
#X text 70 121 Inlet: 0/1 to switch off or on. Default is on. Switch
it off to save some CPU cycles.;
#X obj 80 193 m_accel_pitch;
#X text 65 69 m_accel_pitch watches the force sensor's output and calculates
the pitching of the device (iPod \, iPhone \, ...).;
#X text 47 32 m_accel_pitch - calulate device pitch from accelerometer
;
#X connect 0 0 3 0;
#X connect 3 0 1 0;
