#N canvas 326 55 693 430 10;
#X obj 73 44 inlet~;
#X obj 72 335 outlet~;
#N canvas 263 13 762 384 banghold~ 0;
#X obj 101 280 samphold~;
#X obj 162 255 vline~;
#X obj 205 100 samplerate~;
#X obj 205 122 swap 1000;
#X obj 205 147 /;
#X obj 205 69 loadbang;
#X obj 162 198 f;
#X msg 162 230 -1 \, 0 0 \$1;
#X obj 162 41 inlet;
#X obj 162 177 b;
#X obj 102 41 inlet~;
#X obj 101 304 outlet~;
#X msg 289 69 bang;
#X text 234 24 samples its input whenever it receives a bang at the
first inlet. Accurate up to one sample duration.;
#X connect 0 0 11 0;
#X connect 1 0 0 1;
#X connect 2 0 3 0;
#X connect 3 0 4 0;
#X connect 3 1 4 1;
#X connect 4 0 6 1;
#X connect 5 0 2 0;
#X connect 6 0 7 0;
#X connect 7 0 1 0;
#X connect 8 0 9 0;
#X connect 9 0 6 0;
#X connect 10 0 0 0;
#X connect 12 0 2 0;
#X restore 89 127 pd banghold~;
#X obj 71 165 -~;
#X obj 71 297 wrap~;
#X obj 71 240 +~;
#X obj 72 81 phasor~;
#X obj 170 43 inlet;
#X obj 202 206 vline~;
#X obj 202 95 wrap;
#N canvas 228 198 627 317 LICENSE-BSD 0;
#X text 121 56 This software is copyrighted by Miller Puckette \, Reality
Jockey Ltd. and others. The terms (the "Standard Improved BSD License")
apply to all files associated with the software unless explicitly disclaimed
in individual files.;
#X text 123 148 See the file LICENSE.txt for the full license text.
;
#X restore 233 40 pd LICENSE-BSD;
#X obj 202 177 + 2;
#X obj 170 67 t b f;
#X text 235 177 workaround for a bug in [wrap~] which converts 0 to
1;
#X connect 0 0 6 0;
#X connect 2 0 3 1;
#X connect 3 0 5 0;
#X connect 4 0 1 0;
#X connect 5 0 4 0;
#X connect 6 0 3 0;
#X connect 6 0 2 0;
#X connect 7 0 12 0;
#X connect 8 0 5 1;
#X connect 9 0 11 0;
#X connect 11 0 8 0;
#X connect 12 0 2 1;
#X connect 12 1 9 0;
