# Viewing Multihost session information using EDM

Use the following procedure to view multiple host session information for a port.

Important

The Multi Hosts and Non-EAP MAC buttons are not available when configuring multiple ports on the EAPOL Advance tab. To make use of these two options, you can select only one port.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

   The Port tab appears.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Multi Host.

   The Multi Host, Port tab appears.

6. In the work area, click the Multi Host Session tab to view multi host session information.

## Variable definitions

Use the data in the following table to view Multihost session information.

Variable | Value
--- | ---
PortNumber | Specifies the port number in use.
ClientMACAddr | Specifies the MAC address of the client.
Id | Specifies a unique identifier for the session, in the form of a printable ASCII string of at least three characters.
AuthenticMethod | Specifies the authentication method used to establish the session.
Time | Specifies the elapsed time of the session.
TerminateCause | Specifies the cause of the session termination.
UserName | Specifies the user name representing the identity of the supplicant PAE machine.