# Configuring Stack Monitor using EDM

Use the following procedure to configure Stack Monitor using EDM.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure Steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Chassis.

3. In the Chassis tree, double-click Chassis.

4. In the work area, click the Stack Monitor tab.

5. In the Stack Monitor tab, configure the required parameters.

6. On the toolbar, click Apply.

## Variable definitions

The following table describes the fields of Stack Monitor tab.

Field | Description
--- | ---
StackErrorNotificationEnabled | Enables or disables the Stack Monitoring feature.
ExpectedStackSize | Specifies the size of the stack to monitor. Valid range is 2–8. Default value is 2.
StackErrorNotificationInterval | Specifies the time interval between traps, in seconds. Valid range is 30–300 seconds. Default value is 60.
StackRebootUnitOnFailure | Enables or disables the rebooting stack units on failure.
StackRetryCount | Sets the retry count for the stack.