# Graphing VLAN DHCP statistics using EDM

Use the following procedure to create a graph of VLAN DHCP configuration.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. In the VLAN tree, double-click VLANs.

3. In the work area, select the desired VLAN.

4. In the toolbar, click IP.

   The IP, VLAN 1 tab appears.

5. In the work area, click the DHCP tab.

6. In the toolbar, click Graph.

   The DHCP-Graph tab appears.

7. In the work area, highlight the required data.

8. In the toolbar, click the type of graph you want to produce.

## Variable definitions

The following table explains the fields found on this window.

Field | Description
--- | ---
NumRequests | Indicates the number of DHCP requests handled.
NumReplies | Indicates the number of DHCP replies handled.