# Viewing and graphing the EAPOL Diag tab using EDM

Use the following procedure to view read-only EAPOL diagnostic statistics.

## Procedure steps

1. In the Device Physical View, select one or multiple ports.

2. From the navigation tree, double-click Graph.

3. In the Graph tree, double-click Port.

4. In the work area, click the EAPOL Diag tab to view information about EAPOL diagnostic statistics.

## Variable definitions

The following table describes the fields of EAPOL Diag tab.

Field | Description
--- | ---
EntersConnecting | Counts the number of times that the Authenticator PAE state machine transitions to the Connecting state from another state.
EapLogoffsWhileConnecting | Counts the number of times that the Authenticator PAE state machine transitions from Connected to Disconnected as a result of receiving an EAPOL-Logoff message.
EntersAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Connecting to Authenticating as a result of receiving an EAP-Response/Identity message from the supplicant.
AuthSuccessWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Authenticated as a result of the Backend authentication state machine indicating successful authentication of the supplicant.
AuthTimeoutsWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Aborting as a result of the Backend authentication state machine indicating authentication timeout.
AuthFailWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Held as a result of the Backend authentication state machine indicating authentication failure.
AuthReauthsWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Aborting as a result of a reauthentication request.
AuthEapStartsWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Aborting as a result of an EAPOL-Start message being received from the supplicant.
AuthEapLogoffWhileAuthenticating | Counts the number of times that the Authenticator PAE state machine transitions from Authenticating to Aborting as a result of an EAPOL-Logoff message being received from the supplicant.
AuthReauthsWhileAuthenticated | Counts the number of times that the Authenticator PAE state machine transitions from Authenticated to Connecting as a result of a reauthentication request.
AuthEapStartsWhileAuthenticated | Counts the number of times that the Authenticator PAE state machine transitions from Authenticated to Connecting as a result of an EAPOL-Start message being received from the supplicant.
AuthEapLogoffWhileAuthenticated | Counts the number of times that the Authenticator PAE state machine transitions from Authenticated to Disconnected as a result of an EAPOL-Logoff message being received from the supplicant.
BackendResponses | Counts the number of times that the Backend Authentication state machine sends an Initial-Access request packet to the Authentication server.
BackendAccessChallenges | Counts the number of times that the Backend Authentication state machine receives an Initial-Access challenge packet from the Authentication server.
BackendOtherRequestsToSupplicant | Counts the number of times that the Backend Authentication state machine sends an EAP request packet (other than an Identity, Notification, failure, or success message) to the supplicant.
BackendNonNakResponsesFromSupplicant | Counts the number of times that the Backend Authentication state machine receives a response from the supplicant to an initial EAP request and the response is something other than EAP-NAK.
BackendAuthSuccesses | Counts the number of times that the Backend Authentication state machine receives an EAP-success message from the Authentication server.
BackendAuthFails | Counts the number of times that the Backend Authentication state machine receives an EAP-failure message from the Authentication server.