# Viewing LLDP neighbor PoE PD properties

Use this procedure to view LLDP PoE PD properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Neighbor PoE PD tab.

The following table outlines the parameters of the Port MED Neighbor PoE PD tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Identifies a particular MSAP, using an arbitrary local integer value. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
PDPowerReq | Specifies the value of the power required (in units of 0.1 watts) by a Powered Device (PD) connected remotely to the port.
PDPowerSource | Defines the type of Power Source advertised as being used by the remote device: fromPSE: indicates that the device advertises its power source as received from a PSE. local: indicates that the device advertises its power source as local. localAndPSE: indicates that the device advertises its power source as using both local and PSE power.
PDPowerPriority | Defines the priority advertised as being required by the PD connected remotely to the port: critical: indicates that the device advertises its power priority as critical, see RFC 3621. high: indicates that the device advertises its power priority as high, see RFC 3621. low: indicates that the device advertises its power priority as low, see RFC 3621.