# Configuring EAPOL globally using EDM

Use the following procedure to configure EAPOL parameters globally for the switch.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click 802.1X/EAP.

3. In the work area, click the EAPOL tab.

4. Configure the parameters as required.

5. In the toolbar, click Apply.

## Variable definitions

The following table describes the fields of EAPOL tab.

Variable | Value
--- | ---
DefaultEapAll | Restores all EAP settings globally.
SystemAuthControl | Enables or disables port access control on the switch.
UserBasedPolicies Enabled | Enables or disables EAPOL user-based policies. For more information about user-based policies, see Configuring Quality of Service on Avaya Ethernet Routing Switch 5000 Series, NN47200-504.
UserBasedPoliciesFilterOnMac | Enables or disables the filter on MAC addresses for user-based policies.
GuestVlanEnabled | Enables or disables the Guest VLAN.
GuestVlanId | Sets the VLAN ID of the Guest VLAN.
MultiHostAllow NonEapClient | Enables or disables support for non-EAPOL hosts on EAPOL-enabled ports.
MultiHostSingle AuthEnabled | Enables or disables Multiple Host Single Authentication (MHSA). When selected, non-EAPOL hosts are allowed on a port if there is one authenticated EAPOL client on the port.
MultiHostRadiusAuth NonEapClient | Enables or disables RADIUS authentication of non-EAPOL hosts on EAPOL-enabled ports.
MultiHostAllowNonEapPhones | Enables or disables Avaya IP Phone clients as another non-EAP type.
MultiHostAllowRadiusAssignedVlan | Enables or disables the use of RADIUS-assigned VLAN values in the Multihost mode.
MultiHostAllowNonEapRadiusAssignedVlan | Enables or disables the use of non-EAP RADIUS-assigned VLAN values in the Multihost mode.
MultiHostUseMostRecentRadiusAssignedVlan | Enables or disables the use of the most recent VLAN values assigned by the RADIUS server.
MultiHostMultiVlan | Enables or disables the multiple VLAN capability for EAP and non-EAP hosts The default is disabled.
MultiHostEapPacketMode | Enables or disables the choice of packet mode (unicast or multicast) in the Multihost mode. Default is multicast.
MultiHostEapProtocolEnabled | Enables or disables the processing of EAP protocol packets.
MultiHostFailOpenVlanEnabled | Enables or disables the fail-over Vlan.
MultiHostFailOpenVlanId | Specifies the ID of the global fail-over Vlan.
MultiHostFailOpenVlanContinuityModeEnabled | Enables or disables Fail Open VLAN Continuity mode.
NonEapRadiusPasswordAttributeFormat | Enables or disables setting the format of the Remote Authentication Dial-In User Service (RADIUS) Server password attribute for non-EAP clients.
MultiHostNonEapRadiusPasswordFreeformKey | Specifies the RADIUS password key.
Confirm MultiHostNonEapRadiusPasswordFreeformKey | Confirms the RADIUS password key.
NonEapUserBasedPoliciesEnabled | Enables or disables non-EAP user-based policies.
NonEapUserBasedPoliciesFilterOnMac | Enables or disables the filter on MAC addresses for non-EAP user-based policies.
MultiHostNeapReauthenticationEnabled | Enables or disables NEAP reauthentication.
MultiHostBlockDifferentVlanAuth | Enables or disables the block subsequent MAC authentication feature.