# NNS_G2dEntryNewOamEx

## C Specification

      #include <nnsys/g2d/g2d_OAMEx.h>

      BOOL NNS_G2dEntryNewOamEx(
              NNSG2dOamManagerInstanceEx*     pMan,
              const GXOamAttr*                pOam,
              u8                              priority );

## Arguments

`pMan` | [OUT] Extended OAM manager entity
pOam | [IN] OAM attribute
priority | [IN] Display priority (order of registration for drawing)

## Return Values

Success or failure of registration

## Description

Registers OBJs in the extended OAM Manager and specifies the order of the entry when it is drawn. When actually applied to the hardware, this will register to the OAM in the designated display priority order. The name of this function has changed to `NNS_G2dEntryOamManExOam`. In order to maintain compatibility, the previous function was kept under a different name.

## See Also

`NNS_G2dEntryOamManExOam`, `NNS_G2dEntryOamManExOamWithAffineIdx`

## Revision History

08/02/2004 Renamed function

06/22/2004 Initial version