# MI_SetCartridgeRomCycle2nd

## C Specification

  `#include <nitro/mi.h>`
  `void MI_SetCartridgeRomCycle2nd( MICartridgeRomCycle2nd c2 )`

## Description

Sets the 2nd access cycle for access to the Game Pak's ROM region.

The 1st access cycle is set using the function `MI_SetCartridgeRomCycle1st`.

The values for the c2 argument take the form of `MIRomCycle2nd`. The meanings are shown below.

`MI_CTRDG_ROMCYCLE2_4` | 4 cycles
`MI_CTRDG_ROMCYCLE2_6` | 6 cycles

## Arguments

c2 | The 2nd access cycle for access to the Game Pak's ROM region.

## Return Values

None.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRomCycle1st, MI_GetCartridgeRomCycle1st, MI_GetCartridgeRomCycle2nd`

## Revision History

07/01/2004 Name changed from "2" to "2nd"
05/25/2004 Added "cartridge" to name
12/18/2003 Initial version