# MI_WriteByte

## C Specification

  `#include <nitro/mi.h>`
  `void MI_WriteByte( void* address, u8 data )`

## Description

This function writes byte data to the address specified by a void typed pointer.

Internally, it accesses memory as u16 data. Therefore at assembler level, byte access instructions such as `strb/ldrb` will not be generated.

## Arguments

address | Address for writing byte data (pointer)
data | Data to write

## Return Values

None

## See Also

`MI_ReadByte`

## Revision History

03/30/2004 Initial Version