# MB_CommStartSending

## C Specification

      #include <nitro/mb.h>

      BOOL MB_CommStartSending( u16 child_aid );

## Description

This function sends the download start notification from the current parent device to a specific child.

When the parent communication status is `MB_COMM_PSTATE_REQ_WAIT_TO_SEND`, it indicates that a child is waiting for the download start notification.

## Arguments

`child_aid` | The `aid` that tells the child to send the download start notification.

## Return Values

This function returns a value of TRUE if there is a child device that has received connection permissions; the function returns FALSE otherwise.

## See Also

`MBCommPState, MB_CommStartSendingAll, MB_CommGetParentState, MB_CommGetChildUser, MB_CommResponseRequest, MB_StartParent, MB_End`

## Revision History

10/18/2004 Corrected the parent state to MB_COMM_PSTATE_REQ_WAIT_TO_SEND.
09/10/2004 Added a description.
09/09/2004 Added an argument.
08/27/2004 Initial version.