# CARD_TryWaitRomAsync

## C Specification

      #include <nitro/card.h>

      BOOL CARD_TryWaitRomAsync(void);

## Description

Determines whether or not an asynchronous process to a ROM device is complete.

Regardless of the status of the target process, the function immediately returns a value.

## Arguments

None.

## Return Values

Returns `FALSE` if an asynchronous function that operates on a CARD ROM device is actively calling and processing is not yet complete. Otherwise it returns `TRUE`.

## See Also

`CARD_ReadRomAsync, CARD_WaitRomAsync`

## Revision History

07/05/2004 Initial Version