# GXDLInfo

## C Specification

      #include <nitro/gx/g3.h>

      typedef struct
        u8 *curr_cmd;
      	u32 *curr_param;
      	u32 *bottom;
      	u32 length;
      	BOOL param0_cmd_flg;
      	GXDLInfo;

## Description

This structure provides the arguments for `G3B_***`, `G3C_***`, and other functions that create dynamic display lists.

## Members

The details of each member are as follows:

Member | Meaning
`curr_cmd` | Pointer to the position to insert the command.
`curr_param` | Pointer to the position to insert the command parameter.
`bottom` | Pointer to the tail end of the display list.
`length` | Size of the display list.
`param0_cmd_flg` | Parameter to deal with a hardware bug when sending the parameter0 geometry command.

## See Also

`None.`

## Revision History

11/05/2004 Initial version.