# TP_GetLatestRawPointInAuto

## C Specification

  `#include <nitro/spi.h>`

      void TP_GetLatestRawPointInAuto( TPData * result );

## Description

This function selects the most recent valid touch panel values from autosampling results and acquires them. For x, y coordinate values, it takes values in the uncalibrated range (0 – 4095).

## Arguments

`result` | A pointer used for acquiring results

## Return Values

None

## See Also

`

`TPData`, `TP_GetLatestCalibratedPointInAuto`, `TP_RequestAutoSamplingStart`

`

## Revision History

04/16/2004 Initial version