# GX_VBlankIntr

## C Specification

      #include <nitro/gx/gx.h>

      void GX_VBlankIntr(BOOL enable);

## Description

If the argument is other than `FALSE`, this function generates a V-Blank interrupt request. If it is `FALSE`, it does not generate one.

## Argument

`enable` | Sets whether to generate a V-Blank interrupt request

## Return Values

None

## See Also

`GX_IsVBlank`, `GX_HBlankIntr`

## Revision History

07/26/2004 Revised description of the return values

01/19/2004 Initial Version