# CARD_WaitRomAsync

## C Specification

      #include <nitro/card.h>

      void CARD_WaitRomAsync(void);

## Description

If an asynchronous process to a CARD ROM device is running, `CARD_WaitRomAsync` waits until it the asynchronous process completes before executing.

If an asynchronous process is not running, `CARD_WaitRomAsync` returns control immediately.

## Arguments

None.

## Return Values

None.

## See Also

`CARD_ReadRomAsync, CARD_TryWaitRomAsync`

## Revision History

07/05/2004 Initial Version