# MIC_StopAutoSampling

## C Specification

  `#include <nitro/spi.h>`

      MICResult MIC_StopAutoSampling( void );

## Description

Stops microphone auto-sampling.

The function issues a request to ARM7 to stop auto-sampling, waits for ARM7 to respond and returns the process result. This is the synchronous version of MIC_StopAutoSamplingAsync.

## Warning

This function waits for a PXI interrupt in order to gain synchrony. Do not call this function if PXI interrupts have been prohibited.

## Arguments

None.

## Return Values

0 if request succeeds.
Non-zero value if request fails.

## See Also

``MIC_StopAutoSamplingAsync`, `MIC_StartAutoSampling`, `MIC_StartAutoSamplingAsync``

## Revision History

06/01/2004 Initial version