# MB_ReadMultiBootParentBssDesc

## C Specification

      #include <nitro/mb.h>

      void MB_ReadMultiBootParentBssDesc(
          WMBssDesc   *p_desc,
          u16         parent_max_size,
          u16         child_max_size,
          BOOL        ks_flag,
          BOOL        cs_flag);

## Description

If called by a multiboot child, this function stores information for connection to specified memory based on parent information retrieved with the `MB_GetMultiBootParentBssDesc` function. The `WMBssDesc` structure stored by this function can be handled the same as parent information retrieved with the `WM_StartScan` function, and can be provided in an argument of the `WM_StartConnect` function.

## Arguments

`p_desc` | pointer to `WMBssDesc` structure storing parent information
`parent_max_size` | maximum send size of MP parent that the connected parent sets by the `WM_SetParentParameter` function. This size must be stipulated and specified with the application beforehand.
`child_max_size` | maximum send size of MP child that the connected parent sets by the `WM_SetParentParameter` function. This size must be stipulated and specified with the application beforehand.
`ks_flag` | key sharing setting flag that the connected parent sets by the `WM_SetParentParameter` function. This setting must be stipulated and specified with the application beforehand.
`cs_flag` | continuous send setting flag that the connected parent sets by the `WM_SetParentParameter` function. This setting must be stipulated and specified with the application beforehand.

## Return Values

## See Also

WM_SetParentParameter, `WM_StartScan`, `WM_StartConnect`, `MB_GetMultiBootParentBssDesc`

## Revision History

10/05/2004 Initial version