# TP_SetCalibrateParam

## C Specification

  `#include <nitro/spi.h>`

      void TP_SetCalibrateParam( const TPCalibrateParam * param );

## Description

This function sets the parameter that is used for calibration.

After you set the parameter with this function, the value will be used by `TP_WaitCalibratedResult`, `TP_GetLatestCalibratedPointInAuto`, `TP_GetCalibratedPoint`, and `TP_GetUnCalibratedPoint`.

If you set NULL, subsequently coordinates will not be converted using calibration. (The default value is NULL.)

## Arguments

`param` | Pointer to the calibration parameter to be set

## Return Values

None

## See Also

`

`TP_WaitCalibratedResult`, `TP_GetLatestCalibratedPointInAuto`, `TP_GetCalibratedPoint`, `TP_GetUnCalibratedPoint`

`

## Revision History

04/16/2004 Initial version