# TP_GetLatestCalibratedPointInAuto

## C Specification

  `#include <nitro/spi.h>`

      void TP_GetLatestCalibratedPointInAuto( TPData * result );

## Description

This function selects the most recent valid touch panel values from the autosampling results and acquires them. For x, y coordinate values, it takes values in the range of the screen coordinates (x coordinate: 0 – 255, y coordinate: 0 – 191) and it is calibrated.

## Arguments

`result` | Pointer used for acquiring results

## Return Values

None

## See Also

`TPData`, `TP_GetLatestRawPointInAuto`, `TP_RequestAutoSamplingStart`

## Revision History

04/16/2004 Initial version