# G3X_SetFifoIntrCond

## C Specification

      #include <nitro/gx/g3x.h>

      void G3X_SetFifoIntrCond(GXFifoIntrCond cond);

## Description

This function sets command FIFO interrupt request generation conditions. Select from these three options: disable interrupt request, interrupt request when under half, interrupt request when empty.

`GX_FIFOINTR_COND_DISABLE` | Disable command FIFO interrupt request
`GX_FIFOINTR_COND_UNDERHALF` | Interrupt request when command FIFO half or less
`GX_FIFOINTR_COND_EMPTY` | Interrupt request when command FIFO is empty

The following are described in the `GXFifoIntrCond` form, type definition.

    typedef enum
    {
        GX_FIFOINTR_COND_DISABLE = 0,
        GX_FIFOINTR_COND_UNDERHALF = 1,
        GX_FIFOINTR_COND_EMPTY = 2
    }
    GXFifoIntrCond;

## Arguments

Command FIFO interrupt request generation conditions.

## Return Values

None

## See Also

## Revision History

01/19/2004 Initial Version